RS38 FW update SOP

0. download and update qualcomn drive.


<https://qualcommusbdrivers.com/downloads/qualcomm-v1-0-10061-1-usb-driver/>

1. PC: Unzip the attached file “platform-tools-latest-windows”.


2. RS38: go to "usb debug mode".

3. RS38: connect usb cable to PC.

4. RS38: Enable “Allow USB Debuggind" & “always allow from this computer”.

****


5.Type “CMD” in the search bar of the unzip folder.




\*After entering CMD it should look like this.

****

6.Type “adb root” then press enter.

****


7.type “adb reboot edl” then press enter.

****


now it’s in download mode.


8.Click “Configuration” to do setups.


###Do not enable Erase All Before Download###



9.Click “Select Port” and select 9008.







10.Select “rawprogram0\_no\_persist.xml, rawprogram2.xml, rawprogram3.xml, rawprogram4.xml, rawprogram5.xml”.

